,Model##other##,Watts##other##,Volts##other##,Phase##other##,FL Amps##other##,HP##other##,Conn Plug##other##,Electric Connection Type##other##
,,,,,,,,
,,,,,,,,
,,,,,,,,
"208 Volts, 4KW",INFHC-5,4000,208,1,19.3,1/2,NEMA L14-30P,120/208V NEUTRAL REQUIRED
"240 Volts, 4KW",INFHC-5,4000,240,1,16.7,1/2,NEMA L14-30P,120/240V NEUTRAL REQUIRED
